**Specification clauses**

*To be read with Preliminaries/General conditions.*

*Single-leaf gate*

**CLD LockMaster SR3 Panic gate. Tested and certified to LPS1175-7 SR3 by LPCB**

• Width: 1480mm x Height: 2335mm - Outward opening ONLY

• Mesh & wire: As Securus

• Posts: 100x100mm RHS, all welded and drilled

prior to hot dip galvanising and polyester powder-coating

to match fencing.

• Gate frame: 60x60mm RHS, all welded and

drilled prior to hot dip galvanising and polyester powder coating

to match fencing.

• Fixings: CLD Rigid Mesh Panel to be fixed to gate with

Security non-removable fixings, hot dip

galvanised and polyester powder-coated to match fencing.

Gates to be fitted with CLD Lockmaster SR3 Security rated locking

mechanism.

• Method of fixing: Set posts in footings 750 x 750 x 750\*\*\*

mm deep, filled to not less than 3/4 depth with concrete,

as clause 620.